Product code
P887
Platea Pro
P887: Pole-mounted system - Large body optical assembly - Warm White - ST1 street optic.
Technical description:
Outdoor luminaire with direct light street optic, designed to use LED lamps. The optical assembly is made of EN1706AC 46100LF aluminium alloy and subjected to a multi-step, pre-treatment process, in which the main phases are degreasing, fluorozirconation (a protective surface film) and sealing (with a nano-structured silane layer). The painting stage consists of a primer and an acrylic paint, cured at 150°C, with a high level of weather and UV ray resistance. With a 5 mm thick tempered sodium-calcium glass cover. When pole-mounted the product can be adjusted by +15°/ -5° and +5°/-15 when side-mounted. High visual comfort. Polymer optic lenses offering high yield and even light distribution. Complete with circuit fitted with Warm White monochrome power LEDs. Extractable control gear connected with quick-coupling connectors. 220-240V ac 50/60Hz DALI  electronic ballast. The optical assembly is fixed to the ceiling or pole-top attachment by two fixing screws. The light flow emitted in the upper hemisphere of the system in the horizontal position is null (in conformity with the strictest standards for the prevention of light pollution). All external screws are made of stainless steel.
Installation:
The floodlight can be installed on the pole-top with a die-cast aluminium single/double attachment for ø60/76/102/120mm poles or a triple attachment for ø102/120 mm poles. Side die-cast aluminium attachment for tapered poles with diameters between ø 46 and ø76.
Colour:
Grey (15)
Weight (Kg):
8.3
Mounting:
wall arm|pole arm|pole-top side entry|pole-top
Wiring:
The product is connected by inserting the mains cables in a push in terminal board. Resistance to mains voltage spikes of up to 10KV. Product perfect watertightness at the power cable entry point is guaranteed by a nickel-plated brass M24x1.5 cable clamp, suitable for cables with a max external 16mm ø (1,5-2.5mm² cross section).
Class II;IK08;IP66
CE;ENEC-03;BIS;EAC;Retilap;NOM;IRAM
Product configuration: P887+VANO
P887: Pole-mounted system - Large body optical assembly - Warm White - ST1 street optic.
VANO: Optical only
Product characteristics:
Total lighting output [Lm]: 9840
Total luminous flux at or above an angle of 90° [Lm]: 0
Total power [W]: 86.5
Emergency luminous flux [Lm]: /
Luminous efficacy [Lm/W]: 113.8
Voltage [V]: -
Life Time: 100,000h - L90 - B10 (Ta 25°C)
Life Time: 100,000h - L90 - B10 (Ta 40°C)
Ambient operating temperature range: from -40°C to 50°C.
Number of optical assemblies: 1
Optical assembly Characteristics Type 1:
Light Output Ratio (L.O.R.) [%]: 100
Number of lamps for optical assembly: 1
Lamp code: LED
Socket: /
ZVEI Code: LED
Ballast losses [W]: 7.5
Nominal power [W]: /
Colour temperature [K]: 3000
Nominal luminous [Lm]: /
CRI: 70
Lamp maximum intensity [cd]: /
Wavelength [Nm]: /
Beam angle [°]: /
MacAdam Step: 3
