Product code
EM92
Underscore InOut
EM92: Top-Bend 16mm version - Warm white LED - 24Vdc - L= 254mm
Technical description:
IP68 1m permanent immersion linear luminaire – with warm white monochrome LEDs – on a 24Vdc flexible white circuit, length L=254mm. The LED circuit is completely  IP68 1m encapsulated with a high-performance polymer sheath that has a white (outside) and milky finish (emission surface): the material allows the device to be installed and used at temperatures: +25°C in water and +45°C in air. Underscore InOut TOP-BEND can be used to create straight lines on flat and curved surfaces. Even, spotfree lighting is guaranteed along the entire strip profile up to the end parts. At one end (not the head), the product is supplied with a single outlet cable L=5000mm. The product is also supplied with stainless steel wires to stop the body from misshaping as this may damage the led circuit. Easy to install and a robust design for difficult environments (for example, it is salt water, UV and solvent resistant). Minimum curving radius 250mm for 16mm TOP-BEND versions. The luminaire technical characteristics conform to EN 60598-1 standards and particular requirements.
Installation:
Surface-mounted (ceiling and wall) using accessories to be ordered separately. The installation accessories available include AISI 316 stainless steel low clips (L=40mm) that are ideal for curved sections.
Colour:
White (01)
Weight (Kg):
0.17
Mounting:
wall arm|wall surface|ceiling surface
Wiring:
24Vdc ±5% LED circuit. Constant voltage ballasts to be ordered separately, both IP20 and IP67 are available and suitable for outdoor installation. DALI 120W 24V dimming interface available (code no. MWP3) or DALI/DMX/1-10V 12-48Vdc 4-channel dimming interface with 6A per channel, (code no. 9639) suitable for both TW LED and white LED versions.
Notes:
Product complete with LED lamp. Six standard lengths are available (254-504-1004-2004-3004-7004mm).             Immersion installation with clips is not
permitted:
- in areas where direct contact with
people or animals is possible;
- inside swimming pools (allowed only
in surrounding areas);
- on pedestrian or vehicular surfaces.
Class III;IK10;IP68
CE;BIS;EAC;Retilap;ENEC Pending
Product configuration: EM92
EM92: Top-Bend 16mm version - Warm white LED - 24Vdc - L= 254mm
Product characteristics:
Total lighting output [Lm]: 91
Total luminous flux at or above an angle of 90° [Lm]: 12
Total power [W]: 1.2
Emergency luminous flux [Lm]: /
Luminous efficacy [Lm/W]: 75.8
Voltage [V]: 24
Life Time: 84,000h - L80 - B10 (Ta 25°C)
Life Time: 84,000h - L80 - B10 (Ta 40°C)
Ambient operating temperature range: from -30°C to 45°C.
Number of optical assemblies: 1
Optical assembly Characteristics Type 1:
Light Output Ratio (L.O.R.) [%]: 100
Number of lamps for optical assembly: 1
Lamp code: LED
Socket: /
ZVEI Code: LED
Ballast losses [W]: 0
Nominal power [W]: /
Colour temperature [K]: 2800
Nominal luminous [Lm]: /
CRI: 80
Lamp maximum intensity [cd]: /
Wavelength [Nm]: /
Beam angle [°]: /
MacAdam Step: 3
